*Designer,*

*Thank you for your interest in HangSafe Hooks.*

*Please call if you need something we didn’t provide with this set of files.*

*Kevin Schauer*

Hook Spacing:

‘HangSafe Coat Racks’ are offered with standard hook spacings:

* + 5 1/3” Spacing
  + 6.4” Spacing
  + 8” Spacing
  + 10 2/3” Spacing
  + 12” Spacing

Standard lengths of racks are mixed and matched to achieve the desired total coat rack length and/or number of hooks. Hook spacing and the 16” OC ‘mounting pockets’ are not interrupted over the full span of the coat rack.

To Specify:

**Division: 10914**

Determine the desired hook spacing, and open the coordinating DWG file. Follow the equation on the drawing.

Specify a stain color from:

<http://www.minwax.com/products/wood_stains/wood_finish.html#Colors>