WALL MOUNTED “HangSafe Outdoor Rack” COAT RACK SYSTEM -
by “HangSafe Hooks”

PART 1 – GENERAL

1. DESCRIPTION: Furnish and install wall mounted “HangSafe Outdoor Racks”
2. RELATED WORK:
	1. CMU / brick / concrete wall: Blocking not required
	2. Stud framed walls: Horizontal blocking is highly recommended.

PART 2 – PRODUCT

1. Manufacturer: HangSafe Hooks – 165 E. Hwy CC - Nixa, MO - 417-725-8900 or 1-888-803-7403, sales@hangsafehooks.com - [www.hangsafehooks.com](http://www.hangsafehooks.com). – Sole source vendor
2. Materials:
	* 1. Hooks: polycarbonate plastic (rounded ends, eased edges, polished), mounted w/ #14 x 2” stainless steel Philips oval head screws & finishing washers.
		2. Mounting Board: solid composite material (1 9/16” ± x 3 ½”±) w/ choice of finish colors – Redwood, Weathered Wood, Cape Cod Grey, and Cedar.
3. Ordering:
	* + 1. Standard lengths of racks are mixed & matched, to achieve the desired length and/or number of hooks. Standard hook spacings are 5 1/3”, 6.4”, 8”, and 10 2/3”.
			2. Shop drawings will be provided (if needed) to communicate exact configurations including stud spacing to mounting hole coordination, and finish treatments.

PART 3 – EXECUTION

 INSTALLATION

1. Locate solid webs in CMU’s or brick, or studs in framed walls.
2. Install racks level, with mounting screws or mounting system (provided per the wall type) and ¼” flat washers in the ¾” diameter mounting pockets. Tighten screws/bolts to eliminate all movement in rack system.
3. Place finishing button in mounting pocket.

**Note:**

Schauer Family Innovations, LLC is the exclusive provider and manufacturer of the HangSafe flat profile coat hook system. The provided product design is the registered trademark of Schauer Family Innovations, LLC.

Any variation in design, modification to or duplication through production is strictly prohibited without the express written consent of Schauer Family Innovations, LLC.